SURVEY SUBMITTAL CHECK LIST

COUNTY:	DATE:

ROUTE:	CHECKED BY:

PE NO.:

GPK NO.:

MICROSTATION FILE NAME:

While in the .dgn file, go to file>new and create a new file (be sure to use seed file “survseed”) and visualize all the elements in this file. While in this new file, look for the following:

A: any survey chains which do not appear to be drawn correctly (for example chains which cross the road or have the wrong color, linestyle or weight).

B: check to see that all property and existing r.o.w. lines and curves and all parcels are geopak elements.

C: that all elements appear to be drawn correctly (correct feature codes used).

Go back to the original .dgn file and check elements by levels. Scan each level for elements which do not belong or have the wrong linestyle, color or weight. Look at the contours using the .tin file received with the project to see that the .tin file contours correctly. Open the .xls file and compare the information with the information (tract numbers, owner names, etc.) Contained in the .dgn file. After checking to see that all information needed on each level is correct, turn on all levels and look to see that the information is readable and clear.